|  |  |
| --- | --- |
|  | |
| Interfaccia 810D |  |
| Connessioni cavo RS 232 V24 da collegare al morsetto X6  posto dietro il pannello operatore | |
|  | |
| |  |  |  |  |  |  |  | | --- | --- | --- | --- | --- | --- | --- | |  | | | | | | | | **Pin** | **Nome** |  | **Pin** | **Name** |  | http://om-entp.com/images/drives/drive_ic_RS232_1.gif | | 1 | DCD |  | 6 | DSR |  | | 2 | RXD |  | 7 | RTS |  | | 3 | TXD |  | 8 | CTS |  | | 4 | DTR |  | 9 | RI |  | | 5 | 1 M |  |  |  |  | | |
|  | |
| |  |  | | --- | --- | | Significato | | | DCD | Data Carrier Detect | | RxD | Receive Data V24 | | TxD | Transmit Data V24 | | RTS | Request To Send | | CTS | Clear To Send | | DTR | Data Terminal Ready | | DSR | Data Send Ready | | RI | Ring Indicator | | 1M | Signal Ground | |  |  | | |
|  | |
| http://om-entp.com/images/drives/drive_ic_RS232_2.gif | |