|  |
| --- |
|   |
| Interfaccia 810D  |  |
| Connessioni cavo RS 232 V24 da collegare al morsetto X6  posto dietro il pannello operatore |
|  |
|

|  |
| --- |
|  |
| **Pin** | **Nome** |  | **Pin** | **Name** |  | http://om-entp.com/images/drives/drive_ic_RS232_1.gif |
| 1 | DCD |  | 6 | DSR |  |
| 2 | RXD |  | 7 | RTS |  |
| 3 | TXD |  | 8 | CTS |  |
| 4 | DTR |  | 9 | RI |  |
| 5 | 1 M |  |   |   |   |

 |
|   |
|

|  |
| --- |
| Significato  |
| DCD | Data Carrier Detect |
| RxD | Receive Data V24 |
| TxD | Transmit Data V24 |
| RTS | Request To Send |
| CTS | Clear To Send |
| DTR | Data Terminal Ready |
| DSR | Data Send Ready |
| RI | Ring Indicator |
| 1M | Signal Ground |
|  |  |

 |
|   |
| http://om-entp.com/images/drives/drive_ic_RS232_2.gif |